IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "output.ifc"
Time stamp: "2026-07-23T12:21:42"
Author: "AdamKozousek"
Organization: "Unknown"
Preprocessor: "GeometryGymIFCcore v0.2.16.0 by Geometry Gym Pty Ltd built 2026-07-07T22:31:30"
Originating system: "IdeaCheckbot v26.0.3.1869"
Authorization: "None"
Application: "IdeaCheckbot v26.0.3.1869" version "v26.0.3.1869" identifier "IdeaCheckbot v26.0.3.1869" by Organization "Geometry Gym Pty Ltd"

People and organizations
  Person "AdamKozousek" of Organization "Unknown"
  Owner history of Person "AdamKozousek" of Organization "Unknown" | application "IdeaCheckbot v26.0.3.1869" version "v26.0.3.1869" identifier "IdeaCheckbot v26.0.3.1869" by Organization "Geometry Gym Pty Ltd" | change ADDED | created 1784802101 (2026-07-23T10:21:41Z) | last modified 1784802101 (2026-07-23T10:21:41Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: RADIAN
  TIMEUNIT: SECOND

Spatial structure
IFCPROJECT "IFC project"
  IFCSITE
    IFCBUILDING "IFC project"
      contains 4 elements
        4 x IFCELEMENTASSEMBLY | names: "Conn-103", "Conn-105", "Conn-106" (+1 more) | parts: 27 IFCPLATE, 20 IFCFASTENER, 9 IFCMECHANICALFASTENER, 8 IFCBEAM, 3 IFCFOOTING

Property sets
  IDEA_MaterialSteelECEN | properties | on 30 objects (27 IFCPLATE, 3 IFCBEAM)
    Coefficient of thermal expansion = 0.000012 (IFCTHERMALEXPANSIONCOEFFICIENTMEASURE)
    Design code = "ECEN" (IFCLABEL)
    Mass Density = 76982.2025 (IFCMASSDENSITYMEASURE)
    Modulus of elasticity = 206000000000.0 (IFCMODULUSOFELASTICITYMEASURE)
    Name = "S275" (IFCLABEL)
    Over strength coefficient for fu = 1.25 (IFCREAL)
    Over strength coefficient for fy = 1.25 (IFCREAL)
    Poisson's ratio = 0.2875 (IFCREAL)
    Shear modulus = 80000000000.0 (IFCSHEARMODULUSMEASURE)
    Specific heat capacity = 0.49 (IFCSPECIFICHEATCAPACITYMEASURE)
    Thermal conductivity = 50.2 (IFCTHERMALCONDUCTIVITYMEASURE)
    Ultimate strength(fu,40) = 430000000.0 (IFCPRESSUREMEASURE)
    Ultimate strength(fu40) = 430000000.0 (IFCPRESSUREMEASURE)
    Yield strength(fy,40) = 275000000.0 (IFCPRESSUREMEASURE)
    Yield strength(fy40) = 275000000.0 (IFCPRESSUREMEASURE)
  IDEA_MaterialSteelECEN | properties | on 5 objects (5 IFCBEAM)
    Coefficient of thermal expansion = 0.000005 (IFCTHERMALEXPANSIONCOEFFICIENTMEASURE)
    Design code = "ECEN" (IFCLABEL)
    Mass Density = 80708.7295 (IFCMASSDENSITYMEASURE)
    Modulus of elasticity = 164375000000.0 (IFCMODULUSOFELASTICITYMEASURE)
    Name = "Steel cables" (IFCLABEL)
    Over strength coefficient for fu = 1.25 (IFCREAL)
    Over strength coefficient for fy = 1.25 (IFCREAL)
    Poisson's ratio = 0.2875 (IFCREAL)
    Shear modulus = 63834951456.3107 (IFCSHEARMODULUSMEASURE)
    Specific heat capacity = 0.49 (IFCSPECIFICHEATCAPACITYMEASURE)
    Thermal conductivity = 50.2 (IFCTHERMALCONDUCTIVITYMEASURE)
    Ultimate strength(fu,40) = 1534000000.0 (IFCPRESSUREMEASURE)
    Ultimate strength(fu40) = 1534000000.0 (IFCPRESSUREMEASURE)
    Yield strength(fy,40) = 1500000000.0 (IFCPRESSUREMEASURE)
    Yield strength(fy40) = 1500000000.0 (IFCPRESSUREMEASURE)
  IDEA_CrossSection | properties | on 4 objects (4 IFCBEAM)
    Mprl shape name = "Cable 18" (IFCLABEL)
    Name = "Cable 18" (IFCLABEL)
    Type = "OneComponentCss" (IFCLABEL)
  IDEA_CrossSection | properties | on 2 objects (2 IFCBEAM)
    Mprl shape name = "CHS_168.3x5.4" (IFCLABEL)
    Name = "CHS_168.3x5.4" (IFCLABEL)
    Type = "CHSPar" (IFCLABEL)
  IDEA_CrossSection | properties | on 1 object (1 IFCBEAM)
    Mprl shape name = "Cable 20" (IFCLABEL)
    Name = "Cable 20" (IFCLABEL)
    Type = "OneComponentCss" (IFCLABEL)
  IDEA_CrossSection | properties | on 1 object (1 IFCBEAM)
    Mprl shape name = "CHS88,4" (IFCLABEL)
    Name = "CHS88,4" (IFCLABEL)
    Type = "CHSPar" (IFCLABEL)
  IDEA_Plate | properties | on 18 objects (18 IFCPLATE)
    Thickness = 0.01 (IFCREAL)
  IDEA_Plate | properties | on 3 objects (3 IFCPLATE)
    Thickness = 0.03 (IFCREAL)
  IDEA_Plate | properties | on 3 objects (3 IFCPLATE)
    Thickness = 0.015 (IFCREAL)
  IDEA_Plate | properties | on 3 objects (3 IFCPLATE)
    Thickness = 0.02 (IFCREAL)
  IDEA_MaterialBoltGrade | properties | on 6 objects (6 IFCMECHANICALFASTENER)
    Coefficient of thermal expansion = 0.0 (IFCTHERMALEXPANSIONCOEFFICIENTMEASURE)
    Mass Density = 0.0 (IFCMASSDENSITYMEASURE)
    Modulus of elasticity = 206000000000.0 (IFCMODULUSOFELASTICITYMEASURE)
    Name = "S275" (IFCLABEL)
    Poisson's ratio = 0.0 (IFCREAL)
    Specific heat capacity = 0.0 (IFCSPECIFICHEATCAPACITYMEASURE)
    Thermal conductivity = 0.0 (IFCTHERMALCONDUCTIVITYMEASURE)
    Ultimate tensile strength = 430000000.0 (IFCPRESSUREMEASURE)
    Yield strength = 275000000.0 (IFCPRESSUREMEASURE)
  IDEA_MaterialBoltGrade | properties | on 3 objects (3 IFCMECHANICALFASTENER)
    Coefficient of thermal expansion = 0.0 (IFCTHERMALEXPANSIONCOEFFICIENTMEASURE)
    Mass Density = 0.0 (IFCMASSDENSITYMEASURE)
    Modulus of elasticity = 210000000000.0 (IFCMODULUSOFELASTICITYMEASURE)
    Name = "4.6" (IFCLABEL)
    Poisson's ratio = 0.0 (IFCREAL)
    Specific heat capacity = 0.0 (IFCSPECIFICHEATCAPACITYMEASURE)
    Thermal conductivity = 0.0 (IFCTHERMALCONDUCTIVITYMEASURE)
    Ultimate tensile strength = 400000000.0 (IFCPRESSUREMEASURE)
    Yield strength = 240000000.0 (IFCPRESSUREMEASURE)
  IDEA_PinGrid | properties | on 4 objects (4 IFCMECHANICALFASTENER)
    Assembly = "Edit of D20 S275" (IFCLABEL)
    Diameter = 0.02 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Hole diameter = 0.022 (IFCPOSITIVELENGTHMEASURE) [METRE]
  IDEA_PinGrid | properties | on 1 object (1 IFCMECHANICALFASTENER)
    Assembly = "Edit of D36 S275" (IFCLABEL)
    Diameter = 0.036 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Hole diameter = 0.039 (IFCPOSITIVELENGTHMEASURE) [METRE]
  IDEA_PinGrid | properties | on 1 object (1 IFCMECHANICALFASTENER)
    Assembly = "Edit of D24 S275" (IFCLABEL)
    Diameter = 0.024 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Hole diameter = 0.026 (IFCPOSITIVELENGTHMEASURE) [METRE]
  IDEA_AnchorGrid | properties | on 3 objects (3 IFCMECHANICALFASTENER)
    Assembly = "M20 4.6" (IFCLABEL)
    Diameter = 0.02 (IFCPOSITIVELENGTHMEASURE) [METRE]
  IDEA_MaterialConcrete | properties | on 3 objects (3 IFCFOOTING)
    Coefficient of thermal expansion = 0.00001 (IFCTHERMALEXPANSIONCOEFFICIENTMEASURE)
    Compressive strength of concrete = 25000000.0 (IFCPRESSUREMEASURE)
    Mass Density = 2500.0 (IFCMASSDENSITYMEASURE)
    Modulus of elasticity = 31475806210.0193 (IFCMODULUSOFELASTICITYMEASURE)
    Name = "C25/30" (IFCLABEL)
    Poisson's ratio = 0.2 (IFCREAL)
    Specific heat capacity = 750.0 (IFCSPECIFICHEATCAPACITYMEASURE)
    Thermal conductivity = 0.8 (IFCTHERMALCONDUCTIVITYMEASURE)
    Time when minimum strength (1MPa) is reached = 43049.14605806 (IFCTIMEMEASURE) [SECOND]
  IDEA_Material | properties | on 20 objects (20 IFCFASTENER)
    Coefficient of thermal expansion = 0.00014 (IFCTHERMALEXPANSIONCOEFFICIENTMEASURE)
    Mass Density = 7850.0 (IFCMASSDENSITYMEASURE)
    Modulus of elasticity = 210000000000.0 (IFCMODULUSOFELASTICITYMEASURE)
    Name = "S 275" (IFCLABEL)
    Poisson's ratio = 0.3 (IFCREAL)
    Specific heat capacity = 0.6 (IFCSPECIFICHEATCAPACITYMEASURE)
    Thermal conductivity = 45.0 (IFCTHERMALCONDUCTIVITYMEASURE)
  IDEA_Weld | properties | on 16 objects (16 IFCFASTENER)
    Throat thickness = 0.005 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Type = "DoubleFillet" (IFCLABEL)
  IDEA_Weld | properties | on 4 objects (4 IFCFASTENER)
    Throat thickness = 0.005 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Type = "FilletRear" (IFCLABEL)