IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "output.ifc"
Time stamp: "2024-09-19T14:16:00"
Author: "AdamKozousek"
Organization: "Unknown"
Preprocessor: "GeometryGymIFCcore v0.2.16.0 by Geometry Gym Pty Ltd built 2024-09-16T15:27:12"
Originating system: "IdeaCheckbot v24.0.5.1382"
Authorization: "None"
Application: "IdeaCheckbot v24.0.5.1382" version "v24.0.5.1382" identifier "IdeaCheckbot v24.0.5.1382" by Organization "Geometry Gym Pty Ltd"

People and organizations
  Person "AdamKozousek" of Organization "Unknown"
  Owner history of Person "AdamKozousek" of Organization "Unknown" | application "IdeaCheckbot v24.0.5.1382" version "v24.0.5.1382" identifier "IdeaCheckbot v24.0.5.1382" by Organization "Geometry Gym Pty Ltd" | change ADDED | created 1726748160 (2024-09-19T12:16:00Z) | last modified 1726748160 (2024-09-19T12:16:00Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: RADIAN
  TIMEUNIT: SECOND

Spatial structure
IFCPROJECT "IFC project"
  IFCSITE
    IFCBUILDING "IFC project"
      contains 18 elements
        18 x IFCELEMENTASSEMBLY | names: "N7", "N1", "N3" (+15 more) | parts: 74 IFCFASTENER, 66 IFCPLATE, 48 IFCBEAM, 26 IFCMECHANICALFASTENER, 4 IFCFOOTING

Property sets
  IDEA_MaterialSteelECEN | properties | on 117 objects (66 IFCPLATE, 48 IFCBEAM, 3 IFCFASTENER)
    Coefficient of thermal expansion = 0.000012 (IFCTHERMALEXPANSIONCOEFFICIENTMEASURE)
    Design code = "ECEN" (IFCLABEL)
    Mass Density = 7850.0 (IFCMASSDENSITYMEASURE)
    Modulus of elasticity = 210000000000.0 (IFCMODULUSOFELASTICITYMEASURE)
    Name = "S 235" (IFCLABEL)
    Over strength coefficient for fu = 1.25 (IFCREAL)
    Over strength coefficient for fy = 1.25 (IFCREAL)
    Poisson's ratio = 0.3 (IFCREAL)
    Shear modulus = 80769230769.2308 (IFCSHEARMODULUSMEASURE)
    Specific heat capacity = 490.0 (IFCSPECIFICHEATCAPACITYMEASURE)
    Thermal conductivity = 50.2 (IFCTHERMALCONDUCTIVITYMEASURE)
    Ultimate strength(fu,40) = 360000000.0 (IFCPRESSUREMEASURE)
    Ultimate strength(fu40) = 360000000.0 (IFCPRESSUREMEASURE)
    Yield strength(fy,40) = 235000000.0 (IFCPRESSUREMEASURE)
    Yield strength(fy40) = 215000000.0 (IFCPRESSUREMEASURE)
  IDEA_CrossSection | properties | on 14 objects (14 IFCBEAM)
    Mprl shape name = "CHS48.3/3.2" (IFCLABEL)
    Name = "CHS48.3/3.2" (IFCLABEL)
    Type = "RolledCHS" (IFCLABEL)
  IDEA_CrossSection | properties | on 12 objects (12 IFCBEAM)
    Mprl shape name = "I220" (IFCLABEL)
    Name = "I220" (IFCLABEL)
    Type = "RolledI" (IFCLABEL)
  IDEA_CrossSection | properties | on 8 objects (8 IFCBEAM)
    Mprl shape name = "I180" (IFCLABEL)
    Name = "I180" (IFCLABEL)
    Type = "RolledI" (IFCLABEL)
  IDEA_CrossSection | properties | on 8 objects (8 IFCBEAM)
    Mprl shape name = "UPE220" (IFCLABEL)
    Name = "UPE220" (IFCLABEL)
    Type = "RolledU" (IFCLABEL)
  IDEA_CrossSection | properties | on 6 objects (6 IFCBEAM)
    Mprl shape name = "CHS76.1/4.0" (IFCLABEL)
    Name = "CHS76.1/4.0" (IFCLABEL)
    Type = "RolledCHS" (IFCLABEL)
  IDEA_Plate | properties | on 58 objects (58 IFCPLATE)
    Thickness = 0.006 (IFCREAL)
  IDEA_Plate | properties | on 8 objects (8 IFCPLATE)
    Thickness = 0.01 (IFCREAL)
  IDEA_MaterialBoltGrade | properties | on 22 objects (22 IFCMECHANICALFASTENER)
    Coefficient of thermal expansion = 0.0 (IFCTHERMALEXPANSIONCOEFFICIENTMEASURE)
    Mass Density = 0.0 (IFCMASSDENSITYMEASURE)
    Modulus of elasticity = 210000000000.0 (IFCMODULUSOFELASTICITYMEASURE)
    Name = "5.6" (IFCLABEL)
    Poisson's ratio = 0.0 (IFCREAL)
    Specific heat capacity = 0.0 (IFCSPECIFICHEATCAPACITYMEASURE)
    Thermal conductivity = 0.0 (IFCTHERMALCONDUCTIVITYMEASURE)
    Ultimate tensile strength = 500000000.0 (IFCPRESSUREMEASURE)
    Yield strength = 300000000.0 (IFCPRESSUREMEASURE)
  IDEA_MaterialBoltGrade | properties | on 4 objects (4 IFCMECHANICALFASTENER)
    Coefficient of thermal expansion = 0.0 (IFCTHERMALEXPANSIONCOEFFICIENTMEASURE)
    Mass Density = 0.0 (IFCMASSDENSITYMEASURE)
    Modulus of elasticity = 210000000000.0 (IFCMODULUSOFELASTICITYMEASURE)
    Name = "8.8" (IFCLABEL)
    Poisson's ratio = 0.0 (IFCREAL)
    Specific heat capacity = 0.0 (IFCSPECIFICHEATCAPACITYMEASURE)
    Thermal conductivity = 0.0 (IFCTHERMALCONDUCTIVITYMEASURE)
    Ultimate tensile strength = 800000000.0 (IFCPRESSUREMEASURE)
    Yield strength = 640000000.0 (IFCPRESSUREMEASURE)
  IDEA_AnchorGrid | properties | on 4 objects (4 IFCMECHANICALFASTENER)
    Assembly = "M16 8.8" (IFCLABEL)
    Diameter = 0.016 (IFCPOSITIVELENGTHMEASURE) [METRE]
  IDEA_MaterialConcrete | properties | on 4 objects (4 IFCFOOTING)
    Coefficient of thermal expansion = 0.00001 (IFCTHERMALEXPANSIONCOEFFICIENTMEASURE)
    Compressive strength of concrete = 30000000.0 (IFCPRESSUREMEASURE)
    Mass Density = 2500.0 (IFCMASSDENSITYMEASURE)
    Modulus of elasticity = 32836568031.3308 (IFCMODULUSOFELASTICITYMEASURE)
    Name = "C30/37" (IFCLABEL)
    Poisson's ratio = 0.2 (IFCREAL)
    Specific heat capacity = 750.0 (IFCSPECIFICHEATCAPACITYMEASURE)
    Thermal conductivity = 0.8 (IFCTHERMALCONDUCTIVITYMEASURE)
    Time when minimum strength (1MPa) is reached = 35962.7245158749 (IFCTIMEMEASURE) [SECOND]
  IDEA_Material | properties | on 71 objects (71 IFCFASTENER)
    Coefficient of thermal expansion = 0.00014 (IFCTHERMALEXPANSIONCOEFFICIENTMEASURE)
    Mass Density = 7850.0 (IFCMASSDENSITYMEASURE)
    Modulus of elasticity = 210000000000.0 (IFCMODULUSOFELASTICITYMEASURE)
    Name = "S 235" (IFCLABEL)
    Poisson's ratio = 0.3 (IFCREAL)
    Specific heat capacity = 0.6 (IFCSPECIFICHEATCAPACITYMEASURE)
    Thermal conductivity = 45.0 (IFCTHERMALCONDUCTIVITYMEASURE)
  IDEA_Weld | properties | on 32 objects (32 IFCFASTENER)
    Throat thickness = 0.003 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Type = "DoubleFillet" (IFCLABEL)
  IDEA_Weld | properties | on 18 objects (18 IFCFASTENER)
    Throat thickness = 0.003 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Type = "FilletRear" (IFCLABEL)
  IDEA_Weld | properties | on 4 objects (4 IFCFASTENER)
    Throat thickness = 0.005 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Type = "DoubleFillet" (IFCLABEL)
  IDEA_Weld | properties | on 4 objects (4 IFCFASTENER)
    Throat thickness = 0.00345000004768372 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Type = "DoubleFillet" (IFCLABEL)
  IDEA_Weld | properties | on 4 objects (4 IFCFASTENER)
    Throat thickness = 0.003 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Type = "Fillet" (IFCLABEL)
  IDEA_Weld | properties | on 4 objects (4 IFCFASTENER)
    Throat thickness = 0.00405000019073486 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Type = "DoubleFillet" (IFCLABEL)
  IDEA_Weld | properties | on 4 objects (4 IFCFASTENER)
    Throat thickness = 0.00325 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Type = "DoubleFillet" (IFCLABEL)
  IDEA_Weld | properties | on 4 objects (4 IFCFASTENER)
    Throat thickness = 0.004 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Type = "DoubleFillet" (IFCLABEL)
  IDEA_BoltGrid | properties | on 22 objects (22 IFCMECHANICALFASTENER)
    Assembly = "M12 5.6" (IFCLABEL)
    Diameter = 0.012 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Hole diameter = 0.013 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Hole slotted = 0.0 (IFCLENGTHMEASURE) [METRE]
    Plane in thread = TRUE (IFCBOOLEAN)