IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "output.ifc"
Time stamp: "2025-05-09T22:47:37"
Author: "AdamKozousek"
Organization: "Unknown"
Preprocessor: "GeometryGymIFCcore v0.2.16.0 by Geometry Gym Pty Ltd built 2025-05-07T17:33:42"
Originating system: "IdeaCheckbot v25.0.1.960"
Authorization: "None"
Application: "IdeaCheckbot v25.0.1.960" version "v25.0.1.960" identifier "IdeaCheckbot v25.0.1.960" by Organization "Geometry Gym Pty Ltd"

People and organizations
  Person "AdamKozousek" of Organization "Unknown"
  Owner history of Person "AdamKozousek" of Organization "Unknown" | application "IdeaCheckbot v25.0.1.960" version "v25.0.1.960" identifier "IdeaCheckbot v25.0.1.960" by Organization "Geometry Gym Pty Ltd" | change ADDED | created 1746823657 (2025-05-09T20:47:37Z) | last modified 1746823657 (2025-05-09T20:47:37Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: RADIAN
  TIMEUNIT: SECOND

Spatial structure
IFCPROJECT "IFC project"
  IFCSITE
    IFCBUILDING "IFC project"
      contains 65 elements
        65 x IFCELEMENTASSEMBLY | names: "23", "27", "34" (+62 more) | parts: 216 IFCBEAM, 70 IFCMECHANICALFASTENER, 12 IFCFASTENER, 6 IFCFOOTING, 6 IFCPLATE

Property sets
  IDEA_MaterialSteelECEN | properties | on 142 objects (136 IFCBEAM, 6 IFCPLATE)
    Coefficient of thermal expansion = 0.000012 (IFCTHERMALEXPANSIONCOEFFICIENTMEASURE)
    Design code = "ECEN" (IFCLABEL)
    Mass Density = 7850.0 (IFCMASSDENSITYMEASURE)
    Modulus of elasticity = 210000000000.0 (IFCMODULUSOFELASTICITYMEASURE)
    Name = "S 355" (IFCLABEL)
    Over strength coefficient for fu = 1.25 (IFCREAL)
    Over strength coefficient for fy = 1.25 (IFCREAL)
    Poisson's ratio = 0.3 (IFCREAL)
    Shear modulus = 80769230769.2308 (IFCSHEARMODULUSMEASURE)
    Specific heat capacity = 490.0 (IFCSPECIFICHEATCAPACITYMEASURE)
    Thermal conductivity = 50.2 (IFCTHERMALCONDUCTIVITYMEASURE)
    Ultimate strength(fu,40) = 490000000.0 (IFCPRESSUREMEASURE)
    Ultimate strength(fu40) = 470000000.0 (IFCPRESSUREMEASURE)
    Yield strength(fy,40) = 355000000.0 (IFCPRESSUREMEASURE)
    Yield strength(fy40) = 335000000.0 (IFCPRESSUREMEASURE)
  IDEA_MaterialSteelECEN | properties | on 80 objects (80 IFCBEAM)
    Coefficient of thermal expansion = 0.000012 (IFCTHERMALEXPANSIONCOEFFICIENTMEASURE)
    Design code = "ECEN" (IFCLABEL)
    Mass Density = 7850.0 (IFCMASSDENSITYMEASURE)
    Modulus of elasticity = 210000000000.0 (IFCMODULUSOFELASTICITYMEASURE)
    Name = "S 275" (IFCLABEL)
    Over strength coefficient for fu = 1.25 (IFCREAL)
    Over strength coefficient for fy = 1.25 (IFCREAL)
    Poisson's ratio = 0.3 (IFCREAL)
    Shear modulus = 80769230769.2308 (IFCSHEARMODULUSMEASURE)
    Specific heat capacity = 490.0 (IFCSPECIFICHEATCAPACITYMEASURE)
    Thermal conductivity = 50.2 (IFCTHERMALCONDUCTIVITYMEASURE)
    Ultimate strength(fu,40) = 430000000.0 (IFCPRESSUREMEASURE)
    Ultimate strength(fu40) = 410000000.0 (IFCPRESSUREMEASURE)
    Yield strength(fy,40) = 275000000.0 (IFCPRESSUREMEASURE)
    Yield strength(fy40) = 255000000.0 (IFCPRESSUREMEASURE)
  IDEA_CrossSection | properties | on 120 objects (120 IFCBEAM)
    Mprl shape name = "UC 305 x 305 x 137" (IFCLABEL)
    Name = "UC 305 x 305 x 137" (IFCLABEL)
    Type = "RolledI" (IFCLABEL)
  IDEA_CrossSection | properties | on 80 objects (80 IFCBEAM)
    Mprl shape name = "UNP200" (IFCLABEL)
    Name = "UNP200" (IFCLABEL)
    Type = "RolledU" (IFCLABEL)
  IDEA_CrossSection | properties | on 16 objects (16 IFCBEAM)
    Mprl shape name = "Rod 20mm" (IFCLABEL)
    Name = "Rod 20mm" (IFCLABEL)
    Type = "OneComponentCss" (IFCLABEL)
  IDEA_Plate | properties | on 6 objects (6 IFCPLATE)
    Thickness = 0.02 (IFCREAL)
  IDEA_MaterialBoltGrade | properties | on 64 objects (64 IFCMECHANICALFASTENER)
    Coefficient of thermal expansion = 0.0 (IFCTHERMALEXPANSIONCOEFFICIENTMEASURE)
    Mass Density = 0.0 (IFCMASSDENSITYMEASURE)
    Modulus of elasticity = 210000000000.0 (IFCMODULUSOFELASTICITYMEASURE)
    Name = "8.8" (IFCLABEL)
    Poisson's ratio = 0.0 (IFCREAL)
    Specific heat capacity = 0.0 (IFCSPECIFICHEATCAPACITYMEASURE)
    Thermal conductivity = 0.0 (IFCTHERMALCONDUCTIVITYMEASURE)
    Ultimate tensile strength = 800000000.0 (IFCPRESSUREMEASURE)
    Yield strength = 640000000.0 (IFCPRESSUREMEASURE)
  IDEA_MaterialBoltGrade | properties | on 6 objects (6 IFCMECHANICALFASTENER)
    Coefficient of thermal expansion = 0.0 (IFCTHERMALEXPANSIONCOEFFICIENTMEASURE)
    Mass Density = 0.0 (IFCMASSDENSITYMEASURE)
    Modulus of elasticity = 210000000000.0 (IFCMODULUSOFELASTICITYMEASURE)
    Name = "4.6" (IFCLABEL)
    Poisson's ratio = 0.0 (IFCREAL)
    Specific heat capacity = 0.0 (IFCSPECIFICHEATCAPACITYMEASURE)
    Thermal conductivity = 0.0 (IFCTHERMALCONDUCTIVITYMEASURE)
    Ultimate tensile strength = 400000000.0 (IFCPRESSUREMEASURE)
    Yield strength = 240000000.0 (IFCPRESSUREMEASURE)
  IDEA_AnchorGrid | properties | on 6 objects (6 IFCMECHANICALFASTENER)
    Assembly = "M24 4.6" (IFCLABEL)
    Diameter = 0.024 (IFCPOSITIVELENGTHMEASURE) [METRE]
  IDEA_MaterialConcrete | properties | on 6 objects (6 IFCFOOTING)
    Coefficient of thermal expansion = 0.00001 (IFCTHERMALEXPANSIONCOEFFICIENTMEASURE)
    Compressive strength of concrete = 25000000.0 (IFCPRESSUREMEASURE)
    Mass Density = 2500.0 (IFCMASSDENSITYMEASURE)
    Modulus of elasticity = 31475806210.0193 (IFCMODULUSOFELASTICITYMEASURE)
    Name = "C25/30" (IFCLABEL)
    Poisson's ratio = 0.2 (IFCREAL)
    Specific heat capacity = 750.0 (IFCSPECIFICHEATCAPACITYMEASURE)
    Thermal conductivity = 0.8 (IFCTHERMALCONDUCTIVITYMEASURE)
    Time when minimum strength (1MPa) is reached = 43049.14605806 (IFCTIMEMEASURE) [SECOND]
  IDEA_Material | properties | on 12 objects (12 IFCFASTENER)
    Coefficient of thermal expansion = 0.00014 (IFCTHERMALEXPANSIONCOEFFICIENTMEASURE)
    Mass Density = 7850.0 (IFCMASSDENSITYMEASURE)
    Modulus of elasticity = 210000000000.0 (IFCMODULUSOFELASTICITYMEASURE)
    Name = "S 355" (IFCLABEL)
    Poisson's ratio = 0.3 (IFCREAL)
    Specific heat capacity = 0.6 (IFCSPECIFICHEATCAPACITYMEASURE)
    Thermal conductivity = 45.0 (IFCTHERMALCONDUCTIVITYMEASURE)
  IDEA_Weld | properties | on 6 objects (6 IFCFASTENER)
    Throat thickness = 0.007 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Type = "DoubleFillet" (IFCLABEL)
  IDEA_Weld | properties | on 6 objects (6 IFCFASTENER)
    Throat thickness = 0.005 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Type = "DoubleFillet" (IFCLABEL)
  IDEA_BoltGrid | properties | on 64 objects (64 IFCMECHANICALFASTENER)
    Assembly = "M14 8.8" (IFCLABEL)
    Diameter = 0.014 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Hole diameter = 0.016 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Plane in thread = TRUE (IFCBOOLEAN)