IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "output.ifc"
Time stamp: "2024-09-06T12:45:03"
Author: "AlexanderSzotkowski"
Organization: "Unknown"
Preprocessor: "GeometryGymIFCcore v0.2.16.0 by Geometry Gym Pty Ltd built 2024-08-30T13:07:38"
Originating system: "IdeaCheckbot v24.0.5.1006"
Authorization: "None"
Application: "IdeaCheckbot v24.0.5.1006" version "v24.0.5.1006" identifier "IdeaCheckbot v24.0.5.1006" by Organization "Geometry Gym Pty Ltd"

People and organizations
  Person "AlexanderSzotkowski" of Organization "Unknown"
  Owner history of Person "AlexanderSzotkowski" of Organization "Unknown" | application "IdeaCheckbot v24.0.5.1006" version "v24.0.5.1006" identifier "IdeaCheckbot v24.0.5.1006" by Organization "Geometry Gym Pty Ltd" | change ADDED | created 1725619503 (2024-09-06T10:45:03Z) | last modified 1725619503 (2024-09-06T10:45:03Z)

Units
  LENGTHUNIT: METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: RADIAN
  TIMEUNIT: SECOND

Spatial structure
IFCPROJECT "IFC project"
  IFCSITE
    IFCBUILDING "IFC project"
      contains 23 elements
        23 x IFCELEMENTASSEMBLY | names: "N1", "N2", "N6" (+20 more) | parts: 80 IFCFASTENER, 69 IFCPLATE, 65 IFCBEAM, 30 IFCMECHANICALFASTENER, 4 IFCFOOTING

Property sets
  IDEA_MaterialSteelECEN | properties | on 134 objects (69 IFCPLATE, 65 IFCBEAM)
    Coefficient of thermal expansion = 0.000012 (IFCTHERMALEXPANSIONCOEFFICIENTMEASURE)
    Design code = "ECEN" (IFCLABEL)
    Mass Density = 7850.0 (IFCMASSDENSITYMEASURE)
    Modulus of elasticity = 210000000000.0 (IFCMODULUSOFELASTICITYMEASURE)
    Name = "S 355" (IFCLABEL)
    Over strength coefficient for fu = 1.25 (IFCREAL)
    Over strength coefficient for fy = 1.25 (IFCREAL)
    Poisson's ratio = 0.3 (IFCREAL)
    Shear modulus = 80769230769.2308 (IFCSHEARMODULUSMEASURE)
    Specific heat capacity = 490.0 (IFCSPECIFICHEATCAPACITYMEASURE)
    Thermal conductivity = 50.2 (IFCTHERMALCONDUCTIVITYMEASURE)
    Ultimate strength(fu,40) = 490000000.0 (IFCPRESSUREMEASURE)
    Ultimate strength(fu40) = 470000000.0 (IFCPRESSUREMEASURE)
    Yield strength(fy,40) = 355000000.0 (IFCPRESSUREMEASURE)
    Yield strength(fy40) = 335000000.0 (IFCPRESSUREMEASURE)
  IDEA_CrossSection | properties | on 19 objects (19 IFCBEAM)
    Mprl shape name = "IPE600" (IFCLABEL)
    Name = "IPE600" (IFCLABEL)
    Type = "RolledI" (IFCLABEL)
  IDEA_CrossSection | properties | on 17 objects (17 IFCBEAM)
    Mprl shape name = "CE 240" (IFCLABEL)
    Name = "CE 240" (IFCLABEL)
    Type = "RolledUPar" (IFCLABEL)
  IDEA_CrossSection | properties | on 13 objects (13 IFCBEAM)
    Mprl shape name = "IPE200" (IFCLABEL)
    Name = "IPE200" (IFCLABEL)
    Type = "RolledI" (IFCLABEL)
  IDEA_CrossSection | properties | on 7 objects (7 IFCBEAM)
    Mprl shape name = "HEB240" (IFCLABEL)
    Name = "HEB240" (IFCLABEL)
    Type = "RolledI" (IFCLABEL)
  IDEA_CrossSection | properties | on 6 objects (6 IFCBEAM)
    Mprl shape name = "IPE240" (IFCLABEL)
    Name = "IPE240" (IFCLABEL)
    Type = "RolledI" (IFCLABEL)
  IDEA_CrossSection | properties | on 3 objects (3 IFCBEAM)
    Mprl shape name = "IASYM_1(Iwn580x(400/250))(Iwn580x(400/250))" (IFCLABEL)
    Name = "Iwn580x(400/250)" (IFCLABEL)
    Type = "Iwn" (IFCLABEL)
  IDEA_Plate | properties | on 36 objects (36 IFCPLATE)
    Thickness = 0.01 (IFCREAL)
  IDEA_Plate | properties | on 12 objects (12 IFCPLATE)
    Thickness = 0.019 (IFCREAL)
  IDEA_Plate | properties | on 8 objects (8 IFCPLATE)
    Thickness = 0.014 (IFCREAL)
  IDEA_Plate | properties | on 5 objects (5 IFCPLATE)
    Thickness = 0.012 (IFCREAL)
  IDEA_Plate | properties | on 4 objects (4 IFCPLATE)
    Thickness = 0.015 (IFCREAL)
  IDEA_Plate | properties | on 2 objects (2 IFCPLATE)
    Thickness = 0.008 (IFCREAL)
  IDEA_Plate | properties | on 2 objects (2 IFCPLATE)
    Thickness = 0.025 (IFCREAL)
  IDEA_MaterialBoltGrade | properties | on 27 objects (27 IFCMECHANICALFASTENER)
    Coefficient of thermal expansion = 0.0 (IFCTHERMALEXPANSIONCOEFFICIENTMEASURE)
    Mass Density = 0.0 (IFCMASSDENSITYMEASURE)
    Modulus of elasticity = 210000000000.0 (IFCMODULUSOFELASTICITYMEASURE)
    Name = "8.8" (IFCLABEL)
    Poisson's ratio = 0.0 (IFCREAL)
    Specific heat capacity = 0.0 (IFCSPECIFICHEATCAPACITYMEASURE)
    Thermal conductivity = 0.0 (IFCTHERMALCONDUCTIVITYMEASURE)
    Ultimate tensile strength = 800000000.0 (IFCPRESSUREMEASURE)
    Yield strength = 640000000.0 (IFCPRESSUREMEASURE)
  IDEA_MaterialBoltGrade | properties | on 3 objects (3 IFCMECHANICALFASTENER)
    Coefficient of thermal expansion = 0.0 (IFCTHERMALEXPANSIONCOEFFICIENTMEASURE)
    Mass Density = 0.0 (IFCMASSDENSITYMEASURE)
    Modulus of elasticity = 210000000000.0 (IFCMODULUSOFELASTICITYMEASURE)
    Name = "10.9" (IFCLABEL)
    Poisson's ratio = 0.0 (IFCREAL)
    Specific heat capacity = 0.0 (IFCSPECIFICHEATCAPACITYMEASURE)
    Thermal conductivity = 0.0 (IFCTHERMALCONDUCTIVITYMEASURE)
    Ultimate tensile strength = 1000000000.0 (IFCPRESSUREMEASURE)
    Yield strength = 900000000.0 (IFCPRESSUREMEASURE)
  IDEA_AnchorGrid | properties | on 4 objects (4 IFCMECHANICALFASTENER)
    Assembly = "M24 8.8" (IFCLABEL)
    Diameter = 0.024 (IFCPOSITIVELENGTHMEASURE) [METRE]
  IDEA_MaterialConcrete | properties | on 4 objects (4 IFCFOOTING)
    Coefficient of thermal expansion = 0.00001 (IFCTHERMALEXPANSIONCOEFFICIENTMEASURE)
    Compressive strength of concrete = 25000000.0 (IFCPRESSUREMEASURE)
    Mass Density = 2500.0 (IFCMASSDENSITYMEASURE)
    Modulus of elasticity = 31475806210.0193 (IFCMODULUSOFELASTICITYMEASURE)
    Name = "C25/30" (IFCLABEL)
    Poisson's ratio = 0.2 (IFCREAL)
    Specific heat capacity = 750.0 (IFCSPECIFICHEATCAPACITYMEASURE)
    Thermal conductivity = 0.8 (IFCTHERMALCONDUCTIVITYMEASURE)
    Time when minimum strength (1MPa) is reached = 43049.14605806 (IFCTIMEMEASURE) [SECOND]
  IDEA_Material | properties | on 80 objects (80 IFCFASTENER)
    Coefficient of thermal expansion = 0.00014 (IFCTHERMALEXPANSIONCOEFFICIENTMEASURE)
    Mass Density = 7850.0 (IFCMASSDENSITYMEASURE)
    Modulus of elasticity = 210000000000.0 (IFCMODULUSOFELASTICITYMEASURE)
    Name = "S 355" (IFCLABEL)
    Poisson's ratio = 0.3 (IFCREAL)
    Specific heat capacity = 0.6 (IFCSPECIFICHEATCAPACITYMEASURE)
    Thermal conductivity = 45.0 (IFCTHERMALCONDUCTIVITYMEASURE)
  IDEA_Weld | properties | on 21 objects (21 IFCFASTENER)
    Throat thickness = 0.004 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Type = "DoubleFillet" (IFCLABEL)
  IDEA_Weld | properties | on 13 objects (13 IFCFASTENER)
    Throat thickness = 0.005 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Type = "DoubleFillet" (IFCLABEL)
  IDEA_Weld | properties | on 10 objects (10 IFCFASTENER)
    Throat thickness = 0.003 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Type = "DoubleFillet" (IFCLABEL)
  IDEA_Weld | properties | on 7 objects (7 IFCFASTENER)
    Throat thickness = 0.006 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Type = "DoubleFillet" (IFCLABEL)
  IDEA_Weld | properties | on 7 objects (7 IFCFASTENER)
    Throat thickness = 0.004 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Type = "Fillet" (IFCLABEL)
  IDEA_Weld | properties | on 6 objects (6 IFCFASTENER)
    Throat thickness = 0.004 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Type = "FilletRear" (IFCLABEL)
  IDEA_Weld | properties | on 3 objects (3 IFCFASTENER)
    Throat thickness = 0.00490000009536743 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Type = "DoubleFillet" (IFCLABEL)
  IDEA_Weld | properties | on 3 objects (3 IFCFASTENER)
    Throat thickness = 0.00309999990463257 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Type = "DoubleFillet" (IFCLABEL)
  IDEA_Weld: 5 more contents on 10 objects not shown
  IDEA_BoltGrid | properties | on 18 objects (18 IFCMECHANICALFASTENER)
    Assembly = "M16 8.8" (IFCLABEL)
    Diameter = 0.016 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Hole diameter = 0.018 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Hole slotted = 0.0 (IFCLENGTHMEASURE) [METRE]
    Plane in thread = TRUE (IFCBOOLEAN)
  IDEA_BoltGrid | properties | on 3 objects (3 IFCMECHANICALFASTENER)
    Assembly = "M16 10.9" (IFCLABEL)
    Diameter = 0.016 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Hole diameter = 0.018 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Hole slotted = 0.0 (IFCLENGTHMEASURE) [METRE]
    Plane in thread = TRUE (IFCBOOLEAN)
  IDEA_BoltGrid | properties | on 3 objects (3 IFCMECHANICALFASTENER)
    Assembly = "M20 8.8" (IFCLABEL)
    Diameter = 0.02 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Hole diameter = 0.022 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Hole slotted = 0.0 (IFCLENGTHMEASURE) [METRE]
    Plane in thread = TRUE (IFCBOOLEAN)
  IDEA_BoltGrid | properties | on 2 objects (2 IFCMECHANICALFASTENER)
    Assembly = "M24 8.8" (IFCLABEL)
    Diameter = 0.024 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Hole diameter = 0.026 (IFCPOSITIVELENGTHMEASURE) [METRE]
    Hole slotted = 0.0 (IFCLENGTHMEASURE) [METRE]
    Plane in thread = TRUE (IFCBOOLEAN)