**Sterilization & Disinfection**

**KynarPure-D can maintain integrity after being exposed to a variety of harsh sterilization methods, for results see table below.**

|  |  |
| --- | --- |
| Autoclave | 124 oC, 30 minutes, 30 Cycles |
| Autoclave | 134 oC, 30 minutes, 20 Cycles |
| Steam in Place | 124 oC, 30 minutes, 30 Cycles |
| Steam in Place | 134 oC, 30 minutes, 20 Cycles |
| Hot Water | 85 oC, 60 minutes, 10 Cycles |

***The common sterilization and disinfection methods above have been tested under controlled laboratory conditions.***

*Note: This Cartridge has a PVDF membrane pre-filter laid over the PVDF membrane final filter and both layers are pleated together.*